Material Safety Data Sheet
CHSM Color

Health		2 
Flammability	3 
Reactivity	0

SECTION I - MANUFACTURER

Air-Tech Coatings, Inc.		Telephone:		1-501-985-1484
#1 Paradise Park Rd.			Toll Free:		1-800-325-1650
Jacksonville, AR  72076		Chemtrec Emergency:  	1-800-535-5053

Products on this MSDS:  	  CHSM Color
OSHA Hazard Class:  		  Paint related materials UN1263
Hazardous Materials Information: See Section 10.
Revised Date:                               10/10/10                           
MSDS Preparation Date:              02/01/05

SECTION II – HAZARDOUS INGREDIENTS
Also see Section X

Ingredients		   CAS#	        Vapor Pressure     SARA 313	              Exposure Limit	  
			                         20 C (MMHg)       Report	    OSHA       ACGH       STEL        CEILING                          
1.  Acrylic Polymer	   Proprietary	N/E	            No   	   None          None        None            None                            
2.  Aluminum		   7429-90-5	None	           Yes	15mg/m3     10mg/m3     N/A                N/A	
3.  Alkyd Resin	                   Proprietary	None                   No	None	None	 None	    None
4.  Bon Maroon		   12225-06-8	N/E	             No	    None	      None         None           None	
5.  Butyl Acetate                    123-86-4           8.40                     No             150 ppm    150 ppm   200 ppm*        ----
6.  Carbon Black		   1333-86-4	None	             No	   3.5mg/m3   3.5mg/m3    N/A             N/A	
7.  Diketopyrrolopyrrol
     Red Pigment		   84632-65-5	None	             No	   None	        None         None           None	      
8.Dioxazine Carbazole
    Pigment		  4378-61-4	None	             No	   15mg/m3     10mg/m3      ----            ----	      
9.  Graphite Synthetic	   Not Available	None	             No	    None          None          None         None	      
10.  Iron Oxide		   1309-37-1	None	             No	    None          10mg/m3      ----           ----	      
11.  Lead Chromate	   18454-12-1	None	           Yes           50ug/m3Pb     50ug/m3Pb       ----           100ug/m3                        						                                 	   50ug/m3Cr    12ug/m3Cr
12.  Lead Chromate 			
       Molybdate		   12656-85-8	None	           Yes	50ug/m3Pb   50ug/m3Pb         ----          100ug/m3           
50ug/m3Cr   12ug/m3Cr
13.  Ferric Hexacyanoferrate14038-43-8	None	            No	 15mg/m3        10mg/m3     ----            ----	        
14.  Methyl Amyl Ketone	   110-43-0	 2.10	            No	  100ppm        100ppm    50ppm         ----	        
15.  Methoxy Propyl Acetate   108-65-6	 3.70	            No	   None              None         ----            ----	        
16.  Methyl Propyl Ketone	   107-87-9	 27.80	            No              200 ppm       200 ppm  250 ppm*      ----	        
17.  Mineral Spirits	8052-41-3      Unknown              No              500 ppm        100 ppm        ----          ----
18.  N Butanol                     	 71-36-3               5.50               Yes              100 ppm         50 ppm        ----     50 ppm skin*
19.  Nickel Antimony 	 8007-18-9           None             Yes             .5mg/m3Sb       .5mg/m3Sb    ----          ----
      Titanium Yellow Pigment	1.0mg/m3N      1.0mg/m3N
20.  Nickel Oxide (Ni)            1313-99-1         None                 Yes             1.0mg/m3             1mg/m3       ----         ----
21.  Perylene Pigment	   128-69-8	None	            No	     ----                10mg/m3       ----          ----	 
22.  Phthalolcyanine Blue							
       Pigment		   147-14-8	None	            No	  15mg/m3         10mg/m3       ----           ----	          
23.  Phthalocyonine Green		
       Pigment	                   1328-53-6	None	            No	  15mg/m3          10mg/m3      ----            ----   	          
24.  Quinacridone Pigment	   1047-16-1	None	            No	  15mg/m3          10mg/m3      ----            ----	
25.  Solvent 100	   	64742-95-6	11.00	            No	  50 ppm	           50 ppm         150ppm    ----	
26.  Titanium Dioxide	   13463-67-7	None	            No 	  15mg/m3         10mg/m3        ----            ----	
27.  Toluene                              108-88-3        36.00                Yes              100 ppm         50 ppm      150 ppm    200 ppm**
28.  Xylene (Note A)	   1330-20-7	25.00	            Yes              100 ppm      100 ppm     150 ppm*      ----    	   

* Denotes 15 Minutes/** Denotes 10 Minutes
Note A:  Technical grade Xylene contains 18-20% Ethylbenzene (100-41-4), which has 100ppm PEL, 100ppm TLV, 125ppm STEL, and is subject to the reporting requirements of Section 313 of Sara Title III.

See Section 5, for specific ingredients and SARA 313 reportable wt.% data.

SECTION III – PHYSICAL DATA
Also see Section X.

Boiling Range:  		2800F – 3020F		Evaporation Rate:  	   Slower than Ether
Solubility in H20:		Very Slight		Vapor Density:		    Heavier than Air
Volatile (%) by Volume:	44.67 – 79.77		Volatile (%) by Weight:	    19.9 – 73.76
Weight per Gallon: 		7.83 – 16.40 lbs./gal.	

SECTION IV – FIRE AND EXPLOSION
Flash Point:  See Section 5.

Flammable Limits:  .8 % - 13%

Extinguishing Media:  Water Spray (for containment), Foam, Carbon Dioxide, Dry Chemical.

Special Fire Fighting Procedures:  Full protective equipment, including self-contained breathing apparatus, is recommended.  Water from fogging nozzles may be used to cool closed containers to prevent pressure build up preventing rupturing.  Do not use direct water stream on combustible or flammable liquid fires.

Unusual fire and explosion hazards:  When heated above the designed flash points these solvents emit flammable vapors which, when mixed with air, can burn or be explosive when exposed to any ignition source.  Fine mists or spray may be flammable at temperatures below the flash point.

SECTION V – HEALTH HAZARD DATA

General Effects:  
Ingestion:  Gastrointestinal distress.  In the unlikely event of ingestion call a physician immediately and have the names of ingredients available.  
Inhalation:  May cause nose and throat irritation.  Repeated and prolonged overexposure to solvents may lead to permanent brain and nervous system damage.  Eye watering, headaches, nausea, dizziness and loss of coordination are signs that solvent levels are too high.  If affected by inhalation of vapor or spray mist, remove to fresh air.  If breathing difficulty persists, or occurs later, consult a physician.
Skin or Eye Contact:  May cause irritation or burning of the eyes.  Repeated or prolonged liquid contact may cause skin irritation with discomfort and dermatitis.  In case of eye contact, immediately flush with plenty of water for at least 15 minutes; call a physician.  In case of skin contact, wash with soap and water.  If irritation occurs, contact a physician. 

Specific Effects:
Lead Chromate, Lead Chromate Molybdate:  Over exposure to lead may cause adverse effects to the blood forming, nervous, urinary, reproductive systems including embryo toxic effects.  Symptoms may include loss of appetite, anemia, disturbance of sleep and fatigue.  See OSHA Lead Standard 29 CFR 1910.1025.  For exposures longer than 8 hours the OSHA exposure limit is reduced by this formula:  limit (in mg/m3)= 400/hours worked in the day.  Lead and Chrome are listed IARC, NPT or OSHA carcinogens.  Warning:  These chemicals are known to the state of California to cause cancer and birth defects or other reproductive harm.
Phthalocyanine Blue Pigment:  Contact may cause skin irritation with discomfort or rash.  Skin permeation can occur in amounts capable of producing the effects of systemic toxicity.
Butyl Acetate: May cause abnormal liver function.
Ethylbenzene:  (Contributed from Xylene) – moderate toxicity by irritation to the skin, eyes, mucous membranes and by ingestion and inhalation routes.  The International Agency for Research on Cancer (IARC) has evaluated ethylbenzene and classified it as a possible human carcinogen (Group 2B) based on sufficient evidence for carcinogenicity in experimental animals, but inadequate evidence for cancer in exposed humans.
Methyl Amyl Ketone:  Ingestion studies on laboratory animals showed that high oral doses caused increased liver and kidney weights.
Methoxy Propyl Acetate:  May cause moderate eye burning.  Continuous over exposures may result in liver and kidney injury.
Mineral Spirits: Laboratory studies with rats have shown that petroleum distillates cause kidney damage and kidney or liver tumors. These effects were seen in similar studies with guinea pigs, dogs, or monkeys. Several studies evaluating petroleum workers have not shown a significant increase of kidney damage or an increase in kidney or liver tumors. May cause temporary upper respiratory and/or lung irritation with cough, difficult breathing, or shortness of breath.
N-Butanol: May cause chemical burns to eyes. May cause abnormal blood forming function with anemia. Reoccurring overexposure may result in liver and kidney injury.
Nickel, Antimony Titanium Yellow:  Antimony and nickel are incorporated into the crystal structure of titanium dioxide.  As such they are chemically and biologically inert.  Material is irritating to the mucous membranes and upper respiratory tract.  Warning:  This chemical is known to the state of California to cause cancer.
Nickel Oxide:  Repeated exposure may cause allergic skin rash, itching, swelling.  Is an IARC, NTP or OSHA carcinogen.  Material is irritating to mucous membranes and upper respiratory tract.  Warning:  This chemical is known to the state of California to cause cancer.
Titanium Dioxide:  In lifetime inhalation tests, lung cancer was found in some rats exposed to 250mg/m3 respirable titanium dust.  Analysis of the titanium dioxide concentrations in the rat’s lungs showed that the lung clearance mechanism was overwhelmed and that the results at the massive 250mg/m3 level are not relevant to the workplace.
Toluene: Reoccurring overexposure may cause liver or kidney damage. High airborne levels have produced irregular heartbeats in animals and occasional palpitations in humans. Rats exposed to very high airborne levels have exhibited  high frequency hearing deficits. Warning: This chemical is known to the state of California to cause birth defects or other reproductive harm.
Xylene:  High concentrations have caused embryo toxic effects in laboratory animals.  Reoccurring overexposure may cause liver or kidney damage.  Can be absorbed through the skin in harmful amounts.

SECTION VI – REACTIVITY DATA
Stability:  Stable
Incompatibility (Materials to avoid):  None reasonable foreseeable. 
Hazardous Decomposition Products:  CO, CO2, Smoke.
Hazardous Polymerization:  Will not occur.

SECTION VII – SPILL OR LEAK PROCEDURES

Steps to be taken in case material is released or spilled:  Ventilate area.  Remove sources of ignition.  Prevent skin contact and breathing of vapor.  Wear a properly fitted vapor/particulate respirator (NIOSH/MSHA TC-23C).  Confine and remove with inert absorbent.
Waste Disposal Method:  Do not allow material to contaminate ground water systems.  Incinerate absorbed material in accordance with federal, state, and local requirements.  Do not incinerate in closed containers.

SECTION VIII – SPECIAL PROTECTION INFORMATION

Do not breathe vapors or mists.  Wear a properly fitted vapor/particulate respirator approved by NIOSH/MSHA (TC-23C) for use with paints during application and until all vapors and spray mists are exhausted.  In confined spaces or in situations where continuous spray operations are typical or proper respirator fit is not possible, wear a positive-pressure, supplied-air respirator (TC-19C).  In all cases, follow the respirator manufacturer’s direction for respirator use.  Do not permit anyone without protection in the painting area.

Ventilation:  Provide sufficient ventilation in volume and pattern to keep contaminants below applicable OSHA requirements.
Protective Clothing:  Neoprene gloves and coveralls are recommended.
Eye Protection:  Desirable in all industrial situations.  Include splashguards or side shields.

SECTION IIIIV – SPECIAL PRECAUTIONS

Precautions to be taken in handling and storing:  Observe label precautions.  Keep away from heat, sparks and flame.  Close container after each use.  Ground containers when pouring. Wash thoroughly after handling and before eating or smoking.  Do not store above 1200F.
Other Precautions:  Do not sand, flame cut, braze or weld dry coating without a NIOSH/MSHA approved respirator or appropriate ventilation.

SECTION X – OTHER INFORMATION
PRODUCT SPECIFICATIONS

For each product part number and chemical listing below the chemicals that have weight percentages in parenthesis are subject to the reporting requirements of Section 313 of the Emergency Planning and Right-To-Know Act of 1986 and 40 CFR 372.

TN1	Acrylic Polymer, Aluminum, Xylene (34%), Solvent 100, Butyl Alcohol (4%), VM&P Naptha, Mineral Spirits 66.
	Gallon Wt.:		8.36 lbs.		Flash Point:		80F
	Wt. % Solids:		51.56			Material VOC:		4.05 lbs/gallon
	Vol. % Solids:		42.36			Coating VOC:		4.05 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.18 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN2	Acrylic Polymer, Aluminum, Xylene (41%), Solvent 100, Butyl Alcohol (1.6%), Mineral Spirits 66.
	Gallon Wt.:		8.51 lbs.		Flash Point:		80F		
	Wt. % Solids:		53.00			Material VOC:		4.0 lbs./gallon
	Vol. % Solids:		44.32			Coating VOC:		4.0 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.20 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN3	Acrylic Polymer, Aluminum, Xylene (40%), Solvent 100, Butyl Alcohol (1.2%), Mineral Spirits 66.
	Gallon Wt.:		8.49 lbs.		Flash Point:		80F
	Wt. % Solids:		54.43			Material VOC:		3.87 lbs./gallon
	Vol. % Solids:		46.11			Coating VOC:		3.87 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.19 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN4	Acrylic Polymer, Aluminum, Xylene (45%), Solvent 100, Butyl Alcohol (1.4%), Mineral Spirits 66.
	Gallon Wt.:		8.54 lbs.		Flash Point:		80F
	Wt. % Solids:		49.29			Material VOC:		4.33 lbs./gallon
	Vol. % Solids:		40.10			Coating VOC:		4.33 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.20 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN5	Acrylic Polymer, Aluminum, Xylene (37%), Solvent 100, Butyl Alcohol (1.6%),Mineral Spirits 66.
	Gallon Wt.:		8.68 lbs.		Flash Point:		80F
	Wt. % Solids:		57.15			Material VOC:		3.72 lbs./gallon
	Vol. % Solids:		48.13			Coating VOC:		3.72 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.18 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN6	Acrylic Polymer, Aluminum, Xylene (40%), Solvent 100, Butyl Alcohol (1.6%), Mineral Spirits 66.
	Gallon Wt.:		8.59 lbs.		Flash Point:		80F
	Wt. % Solids:		53.26			Material VOC:		4.01 lbs./gallon
	Vol. % Solids:		43.85			Coating VOC:		4.01 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.20 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN8	Acrylic Polymer, Aluminum, Xylene (38%), Solvent 100, Butyl Alcohol (1.6%), Mineral Spirits 66.
	Gallon Wt.:		8.79 lbs.		Flash Point:		80F
	Wt. % Solids:		55.77			Material VOC:		3.89 lbs./gallon
	Vol. % Solids:		45.78			Coating VOC:		3.89 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.20 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------

TN21	Acrylic Polymer, Xylene (29.6%), Lead Chromate (48.2%).
	Gallon Wt.:		13.41 lbs.		Flash Point:		80F
	Wt. % Solids:		70.40			Material VOC:		3.97 lbs./gallon
	Vol. % Solids:		45.17			Coating VOC:		3.97 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN22	Acrylic Polymer, Xylene (32.22%),Nickel Antimony Titanium Yellow (43%), Nickel Oxide (2%).
	Gallon Wt.:		10.78 lbs.		Flash Point:		80F
	Wt. % Solids:		64.78			Material VOC:		3.80 lbs./gallon
	Vol. % Solids:		43.54			Coating VOC:		3.80 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN23	Acrylic Polymer, Aluminum, Xylene (38.93%),Iron Oxide.
	Gallon Wt.:		9.41 lbs.		Flash Point:		80F
	Wt. % Solids:		61.07			Material VOC:		3.66 lbs./gallon
	Vol. % Solids:		49.31			Coating VOC:		3.66 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN25	Acrylic Polymer, Xylene (29.5%),Lead Chromate (48.3%)
	Gallon Wt.:		13.38 lbs.		Flash Point:		80F
	Wt. % Solids:		70.5			Material VOC:		3.95 lbs./gallon
	Vol. % Solids:		45.48			Coating VOC:		3.95 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN26	Acrylic Polymer, Xylene (32.22%), Nickel Antimony Titanium Yellow (43%), Nickel Oxide (2%).
	Gallon Wt.:		10.99 lbs.		Flash Point:		80F
	Wt. % Solids:		67.88			Material VOC:		3.53 lbs./gallon
	Vol. % Solids:		46.58			Coating VOC:		3.53 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN27	Acrylic Polymer, Xylene (30.49%), Iron Oxide.
	Gallon Wt.:		11.13 lbs.		Flash Point:		80F
	Wt. % Solids:		69.51			Material VOC:		3.39 lbs./gallon
	Vol. % Solids:		53.13			Coating VOC:		3.39 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN28LS  Acrylic Polymer, Xylene (40.61%), Iron Oxide.
	Gallon Wt.:		8.75 lbs.		Flash Point:		80F
	Wt. % Solids:		59.39			Material VOC:		3.55 lbs./gallon
	Vol. % Solids:		50.72			Coating VOC:		3.55 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN29	Nickel Antimony Titanium Yellow, Titanium Dioxide Acrylic Polymer, Xylene (11%), Methoxy Propyl Acetate
	Gallon Wt.:		17.35 lbs.		Flash Point:		80F
	Wt. % Solids:		80.84			Material VOC:		3.32 lbs./gallon
	Vol. % Solids:		56.00			Coating VOC:		3.32 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.54 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN41	Acrylic Polymer, Xylene (51.63%), Phthalocyanine Blue Pigment
	Gallon Wt.:		 8.52lbs.		Flash Point:		80F
	Wt. % Solids:		48.37			Material VOC:		4.40 lbs./gallon
	Vol. % Solids:		39.20			Coating VOC:		4.40 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN44	Acrylic Polymer, Xylene (57%), Dioxazine Carbazole Pigment.
	Gallon Wt.:		 8.20 lbs.		Flash Point:		80F
	Wt. % Solids:		43.00			Material VOC:		4.67 lbs./gallon
	Vol. % Solids:		35.40			Coating VOC:		4.67 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		

TN45	Acrylic Polymer, Xylene (60%), Phthalocyanine Blue Pigment
	Gallon Wt.:		 8.25 lbs.		Flash Point:		80F
	Wt. % Solids:		39.40			Material VOC:		5.00 lbs./gallon
	Vol. % Solids:		29.70			Coating VOC:		5.00 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN46LS Acrylic Polymer, Xylene (46.97%), Phthalocyanine Blue Pigment
	Gallon Wt.:		 8.18 lbs.		Flash Point:		80F
	Wt. % Solids:		57.03			Material VOC:		3.51 lbs./gallon
	Vol. % Solids:		54.81			Coating VOC:		3.51 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN47	Acrylic Polymer, Xylene (39.78%), Ferric Hexacyanoferrate..
	Gallon Wt.:		 9.46 lbs.		Flash Point:		80F
	Wt. % Solids:		60.22			Material VOC:		3.76 lbs./gallon
	Vol. % Solids:		47.99			Coating VOC:		3.76 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN48	Acrylic Polymer, Xylene (21.60%), Methoxy Propyl Acetate, Phthalocyanine Blue Pigment.
	Gallon Wt.:		 8.69 lbs.		Flash Point:		80F
	Wt. % Solids:		56.67			Material VOC:		3.77 lbs./gallon
	Vol. % Solids:		50.64			Coating VOC:		3.77 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.65 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN49	Acrylic Polymer, Phthalo Blue, Methoxy Propyl Acetate, Xylene (17%), 
	Gallon Wt.:		 8.61 lbs.		Flash Point:		80F
	Wt. % Solids:		47.37			Material VOC:		4.53 lbs./gallon
	Vol. % Solids:		41.70			Coating VOC:		4.53 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.76 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN60	Acrylic Polymer, Xylene (46.4%), Quinacridone Pigment
	Gallon Wt.:		 8.40 lbs.		Flash Point:		80F
	Wt. % Solids:		53.60			Material VOC:		3.90lbs./gallon
	Vol. % Solids:		45.56			Coating VOC:		3.90 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN62	Acrylic Polymer, Organic Magenta, Xylene (20%), Methoxy Propyl Acetate, Butyl Acetate
	Gallon Wt.:		 8.60 lbs.		Flash Point:		80F
	Wt. % Solids:		65.0			Material VOC:		3.01 lbs./gallon
	Vol. % Solids:		60.0			Coating VOC:		3.01 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.47 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN81	Acrylic Polymer, Xylene (40.54%), Phthalocyanine Green Pigment.
	Gallon Wt.:		 8.79 lbs.		Flash Point:		80F
	Wt. % Solids:		51.46			Material VOC:		4.29 lbs./gallon
	Vol. % Solids:		39.85			Coating VOC:		4.29 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN82	Acrylic Polymer, Xylene (49.86%), Phthalocyanine Green Pigment
	Gallon Wt.:		 8.79 lbs.		Flash Point:		80F
	Wt. % Solids:		50.14			Material VOC:		4.38 lbs./gallon
	Vol. % Solids:		38.46			Coating VOC:		4.38 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN83  Acrylic Polymer, Xylene (51%) Phthalocyanine Green Pigment.
	Gallon Wt.:		 8.60 lbs.		Flash Point:		80F
	Wt. % Solids:		49.02			Material VOC:		4.38 lbs./gallon
	Vol. % Solids:		38.52			Coating VOC:		4.38 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN85	 Acrylic Polymer, Phthalocyanine Green, Methyl Amyl Ketone.
	Gallon Wt.:		 9.00 lbs.		Flash Point:		80F
	Wt. % Solids:		48.29			Material VOC:		4.61 lbs./gallon
	Vol. % Solids:		34.00			Coating VOC:		4.61 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	6.89 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN101	 Acrylic Polymer, Xylene (39%), Iron Oxide.
	Gallon Wt.:		 9.41 lbs.		Flash Point:		80F
	Wt. % Solids:		61.00			Material VOC:		3.67 lbs./gallon
	Vol. % Solids:		49.21			Coating VOC:		3.67 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN102	 Acrylic Polymer, Xylene (52.96%), Bon Maroon Pigment.
	Gallon Wt.:		 8.31 lbs.		Flash Point:		80F
	Wt. % Solids:		47.04			Material VOC:		4.40 lbs./gallon
	Vol. % Solids:		39.1			Coating VOC:		4.40 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN104	 Acrylic Polymer, Xylene (44.68%), Quinacridone Pigment.
	Gallon Wt.:		 8.50 lbs.		Flash Point:		80F
	Wt. % Solids:		55.32			Material VOC:		3.80 lbs./gallon
	Vol. % Solids:		47.18			Coating VOC:		3.80 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN105	 Acrylic Polymer, Xylene (30.49%), Iron Oxide.
	Gallon Wt.:		11.13 lbs.		Flash Point:		80F
	Wt. % Solids:		69.51			Material VOC:		3.39 lbs./gallon
	Vol. % Solids:		53.02			Coating VOC:		3.39 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN106LS    Acrylic Polymer, Iron Oxide, Xylene (42.07%)
	Gallon Wt.:		 8.70 lbs.		Flash Point:		80F
	Wt. % Solids:		59.93			Material VOC:		3.66 lbs./gallon
	Vol. % Solids:		49.45			Coating VOC:		3.66 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN107	 Acrylic Polymer, Methoxy Propyl Acetate, Mineral Spirits 66, Iron Oxide.
	Gallon Wt.:		16.40  lbs.		Flash Point:		110F
	Wt. % Solids:		80.10			Material VOC:		3.26 lbs./gallon
	Vol. % Solids:		55.33			Coating VOC:		3.26 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.29 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN108	 Acrylic Polymer, Xylene (57%), Perylene Pigment.
	Gallon Wt.:		 8.07 lbs.		Flash Point:		80F
	Wt. % Solids:		43.00			Material VOC:		4.60 lbs./gallon
	Vol. % Solids:		35.50			Coating VOC:		4.60 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN109	 Acrylic Polymer, Xylene (56.05%), Diketopyrrolopyrrol Red Pigment
	Gallon Wt.:		 8.30 lbs.		Flash Point:		80F
	Wt. % Solids:		43.95			Material VOC:		4.65 lbs./gallon
	Vol. % Solids:		34.74			Coating VOC:		4.65 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN110	 Acrylic Polymer,  Methoxy Propyl Acetate, Xylene (21%), Quinacridone Pyrrolopyrrol..
	Gallon Wt.:		 8.43 lbs.		Flash Point:		80F
	Wt. % Solids:		48.20			Material VOC:		4.37 lbs./gallon
	Vol. % Solids:		43.30			Coating VOC:		4.37 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.70 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN111	. Acrylic Polymer,  Methoxy Propyl Acetate, Xylene (21%), Quinacridone Pyrrolopyrrol
	Gallon Wt.:		 8.48 lbs.		Flash Point:		80F
	Wt. % Solids:		45.80			Material VOC:		4.60 lbs./gallon
	Vol. % Solids:		40.10			Coating VOC:		4.60 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.78 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN112	   Acrylic Polymer,  Methoxy Propyl Acetate, Xylene (21%), Diketopyrrolopyrrol
	Gallon Wt.:		 8.47 lbs.		Flash Point:		80F
	Wt. % Solids:		47.70			Material VOC:		4.43 lbs./gallon
	Vol. % Solids:		42.30			Coating VOC:		4.43 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.65 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN113	 Acrylic Polymer,  Quinacridone Pyrrolopyrrol, Xylene (21.5), Methoxy Propyl Acetate..
	Gallon Wt.:		 8.43 lbs.		Flash Point:		80F
	Wt. % Solids:		48.20			Material VOC:		4.37 lbs./gallon
	Vol. % Solids:		43.27			Coating VOC:		4.37 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN115	   Acrylic Resin, Xylene (15%), Butyl Acetate, Iron Oxide.
	Gallon Wt.:		13.26 lbs.		Flash Point:		72F
	Wt. % Solids:		69.79			Material VOC:		4.01 lbs./gallon
	Vol. % Solids:		45.10			Coating VOC:		4.01 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.30 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN119   Acrylic Polymer, Diketopyrrolopyrrol Red, Methoxy Propyl Acetate, Xylene (16%), 
	Gallon Wt.:		 9.24 lbs.		Flash Point:		80F
	Wt. % Solids:		67.65			Material VOC:		2.29 lbs./gallon
	Vol. % Solids:		61.00			Coating VOC:		2.29 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.65 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN122	   Acrylic Polymer, Xylene (29.5%), Lead Chromate Molybdate (48.3%).
	Gallon Wt.:		13.49 lbs.		Flash Point:		80F
	Wt. % Solids:		70.50			Material VOC:		3.98 lbs./gallon
	Vol. % Solids:		45.03			Coating VOC:		3.98 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN123	   Acrylic Polymer, Xylene (32.04%), Nickel Antimony Titanium Yellow (43%), Nickel Oxide (2%).
	Gallon Wt.:		10.99 lbs.		Flash Point:		80F
	Wt. % Solids:		67.96			Material VOC:		3.52 lbs./gallon
	Vol. % Solids:		46.67			Coating VOC:		3.52 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN124	   Acrylic Polymer, Xylene (5%), Lead Chromate Molybdate (54%), Methoxy Propyl Acetate.
	Gallon Wt.:		19.92 lbs.		Flash Point:		80F
	Wt. % Solids:		77.96			Material VOC:		4.39 lbs./gallon
	Vol. % Solids:		44.95			Coating VOC:		4.39 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.80 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN141LS  Acrylic Polymer, Xylene (45.99%), Carbon Black.
	Gallon Wt.:		 8.19 lbs.		Flash Point:		80F
	Wt. % Solids:		54.01			Material VOC:		3.77 lbs./gallon
	Vol. % Solids:		47.78			Coating VOC:		3.77 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.25 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------

TN142  Acrylic Polymer, Xylene (45.45%), Carbon Black.
	Gallon Wt.:		 8.34 lbs.		Flash Point:		80F
	Wt. % Solids:		54.55			Material VOC:		3.79 lbs./gallon
	Vol. % Solids:		47.64			Coating VOC:		3.79 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN143  Acrylic Polymer, Xylene (49.51%), Carbon Black.
	Gallon Wt.:		 8.33 lbs.		Flash Point:		80F
	Wt. % Solids:		50.49			Material VOC:		4.12 lbs./gallon
	Vol. % Solids:		43.03			Coating VOC:		4.12 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN144  Acrylic Polymer, Xylene (73.76%), Graphite Synthetic. 
	Gallon Wt.:		 7.83 lbs.		Flash Point:		80F
	Wt. % Solids:		26.24			Material VOC:		5.78 lbs./gallon
	Vol. % Solids:		20.23			Coating VOC:		5.78 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN145  Acrylic Polymer, Xylene (48.77%), Carbon Black.
	Gallon Wt.:		 8.32 lbs.		Flash Point:		80F
	Wt. % Solids:		51.23			Material VOC:		4.06 lbs./gallon
	Vol. % Solids:		43.95			Coating VOC:		4.06 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.25 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN161  Acrylic Polymer, Xylene (22.73%), Titanium Dioxide.
	Gallon Wt.:		15.61 lbs.		Flash Point:		80F
	Wt. % Solids:		77.27			Material VOC:		3.55 lbs./gallon
	Vol. % Solids:		54.13			Coating VOC:		3.55 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN163  Acrylic Polymer, Methoxy Propyl Acetate, Xylene (47.7%), Titanium Dioxide,
	Gallon Wt.:		 9.00 lbs.		Flash Point:		80F
	Wt. % Solids:		44.60			Material VOC:		4.98 lbs./gallon
	Vol. % Solids:		32.08			Coating VOC:		4.98 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.33 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN165  Acrylic Polymer,  Titanium Dioxide, Methyl Propyl Ketone, Toluene (2.4%), Xylene (14.1%), Mineral Spirits.
	Gallon Wt.:		13.30 lbs.		Flash Point:		50F
	Wt. % Solids:		71.11			Material VOC:		3.87 lbs./gallon
	Vol. % Solids:		44.21			Coating VOC:		3.87 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	6.94 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------
TN200  Acrylic Polymer, Xylene (44.9%).
	Gallon Wt.:		 8.19 lbs.		Flash Point:		80F
	Wt. % Solids:		55.10			Material VOC:		3.68 lbs./gallon
	Vol. % Solids:		49.21			Coating VOC:		3.68 lbs./gallon
	OSHA Storage:	1B			Solvent Density:	7.24 lbs./gallon		
---------------------------------------------------------------------------------------------------------------------------------------------------

Xylene:  	When present it can be assumed 18-20% of the Wt. % reported is Ethylbenzene.
Flash Point:  	Determined by TCC, expressed in degrees Fahrenheit.
Coating VOC:   WS – WW - WEX     Represents VOC per EPA Method 24.
                                            VT – VW - VEX                                                                                                                                                                                                                    Material VOC: 	ws-ww-wex
Where: 	WS = total solvent weight	VEX = volume of exempt solvent
              	WW = weight of water		VW = volume of water
              	WEX = weight of exempt solvent	VT = total volume

                                                                                                                                                                                                                   
Warning:  KEEP THIS AND ALL PAINT RELATED PRODUCTS OUT OF THE REACH OF CHILDREN!

The information contained in this MSDS is based on data from sources considered to be reliable but Air-Tech Coatings, Inc. does not guarantee the accuracy or completeness thereof.  Air-Tech Coatings, Inc. urges each customer or recipient of this MSDS to study it carefully to become aware of and understand the hazards associated with this product.  The reader should consider consulting reference works or individuals who are experts in ventilation, toxicology or fire prevention as necessary or appropriate to use and understand the data in this MSDS.  

Note:  The data on this MSDS relates only to individual components and does not represent the end mixed product.  Read all other Component Material Safety Data Sheets.