MATERIAL SAFETY DATA SHEET

SECTION 1 - PRODUCT AND COMPANY INFORMATION

AIR TECH COATINGS, INC
1 PARADISE PARK ROAD
JACKSONVILLE,  AR 72076
800-325-1650

EMERGENCY PHONE NUMBERS (24 hours/day): 		800-535-5053

TECHNICAL INFORMATION:    800-325-1650
PRODUCT SAFETY/MSDS INFORMATION: 800-325-1650
PRODUCT ID:   PW 1950
PRODUCT NAME: WASH PRIMER
SYNONYMS: N/A
ISSUE DATE: 10/10/10
CUSTOMER PART #/NAME: N/A 				EDITION NO.: 1
CHEMICAL FAMILY: Phenolic Vinyl

EMERGENCY OVERVIEW:

WARNING!      Flammable. Keep away from heat, sparks, flames, and other sources of ignition. Do not smoke. Extinguish all flames and pilot lights. Turn off stoves, heaters, electrical motors, and other sources of ignition during use and until all vapors/odors are gone. CAUSES EYE IRRITATION.CAUSES PRIMARY SKIN IRRITATION.MAY BE ABSORBED THROUGH THE SKIN. PROLONGED OR REPEATED CONTACT MAY CAUSE AN ALLERGIC SKIN REACTION. VAPOR AND/OR SPRAY MIST MAY BE HARMFUL IF INHALED. VAPOR IRRITATES EYES, NOSE, AND THROAT.MAY BE FATAL OR CAUSE BLINDNESS IF SWALLOWED.

This is an overview of acute and physical hazards associated with this product. Please read the entire MSDS for
complete information.
SECTION 2 - COMPOSITION INFORMATION

The following ingredient(s) marked with an "x" are considered hazardous under applicable U.S. OSHA and/or Canadian WHMIS
regulations:

   Material/CAS Number			Percent		Hazardous

ETHYL ALCOHOL				40 - 70 		      X
        64-17-5
PROPYLENE GLYCOL			   5 - 10 		      X
MONOMETHYL ETHER
       107-98-2
TOLUENE				    3 - 7 		      X
      108-88-3
PHENOLIC RESIN				    3 - 7 		      X
    9003-35-4
ISOBUTYL ALCOHOL			    3 - 7 		     X
        78-83-1
XYLENES				    1 - 5 		     X
      1330-20-7
ETHYL ACETATE				    1 - 5 		     X
       141-78-6
METHYL ALCOHOL			    1 - 5 		     X			
       67-56-1
ZINC TETRA-OXYCHROMATES		    1 - 5 		     X
     13530-65-9
ETHYL BENZENE				   0.1-1.0 		     X
       100-41-4
 (As Chromium (VI) Cmpnds)			       * 		     X		 See Sections 8 and 15 for information.
        13530-65-9
 (As Chromates)				       * 		     X 		See Sections 8 and 15 for information.
        13530-65-9

SECTION 3 - HAZARDS IDENTIFICATION

ACUTE OVEREXPOSURE EFFECTS

EYE CONTACT:
Causes eye irritation. Redness, itching, burning sensation and visual disturbances may indicate excessive eye contact.
SKIN CONTACT:
Causes primary skin irritation. Dryness, itching, cracking, burning, redness, and swelling are conditions associated with excessive skin contact. May be absorbed through the skin. Prolonged or repeated contact may cause an allergic skin reaction.
INHALATION:
Vapor and/or spray mist may be harmful if inhaled. Vapor irritates eyes, nose, and throat.
INGESTION:
May be fatal or cause blindness if swallowed.
SIGNS & SYMPTOMS OF OVEREXPOSURE:
Repeated exposure to high vapor concentrations may cause irritation of the respiratory system and permanent brain and nervous system damage. Eye watering, headaches, nausea, dizziness and loss of coordination are indications that solvent levels are too high. Intentional misuse by deliberately concentrating and inhaling the contents can be harmful or fatal.  Dryness, itching, cracking, burning, redness, and swelling are conditions associated with excessive skin contact.
MEDICAL CONDITIONS AGGRAVATED BY EXPOSURE:
Not applicable.
CHRONIC OVEREXPOSURE EFFECTS
Avoid long-term and repeated contact.  
Repeated exposure to vapors above recommended exposure limits (see Section 8) may cause irritation of the respiratory system and permanent brain and nervous system damage. Intentional misuse by deliberately concentrating and inhaling the contents can be harmful or fatal. This product contains an insoluble form of a chromium (6+) compound. NTP and IARC associate these materials with an increased risk of cancer. This product either contains formaldehyde or is capable of releasing formaldehyde above 0.5 ppm under certain conditions. If this product contains free formaldehyde, formaldehyde will be listed as an ingredient in Section 2 and 11 of this MSDS; if formaldehyde is not specifically listed, this product contains ingredients capable of releasing formaldehyde under certain conditions. Formaldehyde is a potential cancer hazard, a skin sensitizer and a respiratory sensitizer. This product contains toluene. Toluene inhalation in animals (greater than 1500 ppm) and intentional inhalation of toluene-containing products by humans (e.g. glue) has caused adverse fetal development effects. High exposures to xylenes in some animal studies have been reported to cause health effects on the developing embryo and fetus. These effects were often at levels toxic to the mother. The significance of these findings to humans has not been determined.  The effects of long-term, low level exposures to this product have not been determined. Safe handling of this material on a long-term basis should emphasize the prevention of all contact with this material to avoid any effects from repetitive acute exposures. See Section 11, of this MSDS for a detailed list of chronic health effects information available on individual ingredients in this product.

SECTION 4 - FIRST AID MEASURES

If ingestion, irritation, any type of overexposure or symptoms of overexposure occur during or persists after use of this product, contact a POISON CONTROL CENTER, EMERGENCY ROOM OR PHYSICIAN immediately; have Material Safety Data Sheet information available.
EYE CONTACT:
Remove contact lens and pour a gentle stream of warm water through the affected eye for at least 15 minutes. If irritation persists, contact a poison control center, emergency room, or Physician as further treatment may be necessary.
SKIN CONTACT:
SKIN: Run a gentle stream of water over the affected area for 15 minutes. A mild soap may be used if available. If any symptoms persist, contact a poison control center, emergency room, or physician as further treatment may be necessary.

INHALATION:
Remove from area to fresh air. If symptomatic, contact a poison control center, emergency room or physician for
treatment information.
INGESTION:
Gently wipe or rinse the inside of the mouth with water. Sips of water may be given if person is fully conscious. Never give anything by mouth to an unconscious or convulsing person. Do Not induce vomiting. Contact a poison control center, emergency room or physician right away as further treatment will be necessary.

SECTION 5 - FIRE FIGHTING MEASURES

FLAMMABLE PROPERTIES
FLASHPOINT:             40 Degrees F ( 4 Degrees C) FLASHPOINT TEST METHOD: Pensky-Martens Closed Cup
UEL:              Not Available.   			       LEL: 2.9
AUTOIGNITION TEMPERATURE:
Not Available.
EXTINGUISHING MEDIA:
Use National Fire Protection Association (NFPA) Class B extinguishers (carbon dioxide, dry chemical, or universal
aqueous film forming foam) designed to extinguish NFPA Class IB flammable liquid fires. Water spray may be ineffective. Water spray may be used to cool closed containers to prevent pressure build-up and possible auto ignition or explosion when exposed to extreme heat.
PROTECTION OF FIREFIGHTERS:
Fire-fighters should wear self-contained breathing apparatus and full protective clothing.
UNUSUAL FIRE AND EXPLOSION HAZARDS:
Keep this product away from heat, sparks, flame, and other sources of ignition (i.e., pilot lights, electric motors, static electricity). Invisible vapors can travel to a source of ignition and flash back. Do not smoke while using this product. Keep containers tightly closed when not in use. Closed containers may explode when overheated. Do not apply to hot surfaces.  Toxic gases may form when this product comes in contact with extreme heat. May produce hazardous decomposition products when exposed to extreme heat. Extreme heat includes, but is not limited to, flame cutting, brazing, and welding.

SECTION 6 - ACCIDENTAL RELEASE MEASURE

STEPS TO BE TAKEN IF MATERIAL IS RELEASED OR SPILLED:
Provide maximum ventilation. Only personnel equipped with proper respiratory, skin, and eye protection should be
permitted in the area. Remove all sources of ignition. Take up spilled material with sand, vermiculite, or other noncombustible absorbent material and place in clean, empty containers for disposal. Only the spilled material and the absorbent should be placed in this container.

SECTION 7 - HANDLING AND STORAGE

PRECAUTIONS TO BE TAKEN DURING HANDLING AND STORAGE:
Vapors may collect in low areas. If this material is part of a multiple component system, read the Material Safety Data Sheet(s) for the other component or components before blending as the resulting mixture may have the hazards of all of its parts. Containers should be grounded when pouring. Avoid free fall of liquids in excess of a few inches.
STORAGE: Do not store above 120 degrees F.(48 degrees C.). Store large quantities in buildings designed and
protected for storage of NFPA Class IB flammable liquids.

SECTION 8 - EXPOSURE CONTROLS & PERSONAL PROTECTION

ENGINEERING CONTROLS:
Provide general dilution or local exhaust ventilation in volume and pattern to keep the concentration of ingredients listed in Section 8 below the lowest suggested exposure limits, the LEL below the stated limit, and to remove decomposition products during welding or flame cutting.

PERSONAL PROTECTIVE EQUIPMENT
EYES:
Wear chemical-type splash goggles when possibility exists for eye contact due to splashing or spraying liquid, airborne particles, or vapors.
SKIN/GLOVES:
Wear protective clothing sufficient to cover exposed skin surfaces. For applications where skin contact is likely and
impermeable clothing is necessary, select clothing constructed of: butyl rubber. No specific permeation/degradation testing have been done on protective clothing for this product. Recommendations for skin protection are based on infrequent contact with this product. For frequent contact or total immersion, contact a manufacturer of protective clothing for appropriate chemical impervious equipment. Clean contaminated clothing and shoes.
RESPIRATOR:
Overexposure to vapors may be prevented by ensuring proper ventilation controls, vapor exhaust or fresh air entry. A NIOSH- approved air-purifying respirator with the appropriate chemical cartridges or a positive-pressure, air-supplied respirator may also reduce exposure. Read the respirator manufacturer's instructions and literature carefully to determine the type of airborne contaminants against which the respirator is effective, its limitations, and how it is to be properly fitted and used. Provide general dilution or local exhaust ventilation in volume and pattern to keep the concentration of ingredients listed in Section 2 below the lowest suggested exposure limits, the LEL below the stated limit, and to remove decomposition products during welding or flame cutting.
GENERAL HYGIENE - ESTABLISHED EXPOSURE LIMITS

If Threshold Limit Values (TLVs) have been established by ACGIH, OSHA, Ontario or PPG, they will be listed below.  These limits are intended for use in the practice of industrial hygiene as guidelines or recommendations in the control of potential workplace health hazards. These limits are not a relative index of toxicity and should not be used by anyone without industrial hygiene training.

						ACGIH TLV	 ACGIH STEL 	OSHA PEL 	OSHA STEL
  Material/CAS Number		Percent

ETHYL ALCOHOL			40 - 70 		1000 ppm 	Not established 	1000 ppm 	Not established
       64-17-5
PROPYLENE GLYCOL		  5 - 10 		100 ppm 		150 ppm 		100 ppm 		150 ppm
MONOMETHYL ETHER
      107-98-2
TOLUENE			   3 - 7 		S- 50 ppm 	Not established 	100 ppm 		150 ppm
     108-88-3
ISOBUTYL ALCOHOL		   3 - 7 		50 ppm 		Not established 	 50 ppm 		Not established
     78-83-1
XYLENES			   1 - 5 		100 ppm 		150 ppm 		100 ppm 		150 ppm
    1330-20-7
ETHYL ACETATE			   1 - 5 		400 ppm 		Not established 	400 ppm 		Not established
    141-78-6
METHYL ALCOHOL		   1 - 5 		S- 200 ppm 	250 ppm		 S- 200 ppm 	250 ppm
     67-56-1
ZINC TETRA-OXYCHROMATES	   1 – 5		 0.01 mg/m3	 Not established	 C- 0.1 mg/m3	 Not established
     13530-65-9
ETHYL BENZENE			  0.1-1.0		100 ppm 		125 ppm 		100 ppm 		125 ppm
       100-41-4
 (As Chromium (VI) Cmpnds)		   * 		0.05 mg/m3	Not established	 Not established	Not established
      13530-65-9
 (As Chromates)			  * 		Not established	 Not established 	C- 0.1 mg/m3 	Not established 
      13530-65-9

						Ontario TWA 	Ontario STEL 	   PPG IPEL	 PPG STEL
     Material/CAS Number   		Percent

ETHYL ALCOHOL			40 - 70 		1000 ppm	 	Not established	 Not established 	Not established
      64-17-5
PROPYLENE GLYCOL		5 – 10		 100 ppm 		150 ppm		 Not established	 Not established
MONOMETHYL ETHER
    107-98-2
TOLUENE			 3 - 7 		  50 ppm 		150 ppm 		  Not established	 Not established
    108-88-3
ISOBUTYL ALCOHOL		 3 - 7 		   50 ppm 		Not established 	  Not established 	 Not established
      78-83-1
XYLENES			 1 - 5 		100 ppm 		150 ppm 		   Not established 	  Not established
   1330-20-7
ETHYL ACETATE			 1 - 5 		400 ppm		 Not established	   Not established	 Not established
    141-78-6
METHYL ALCOHOL		 1 - 5 		S- 200 ppm 	250 ppm 		    Not established	  Not established
     						Ontario TWA 	Ontario STEL 	   PPG IPEL	 PPG STEL
     Material/CAS Number   		Percent

     67-56-1
ZINC TETRA-OXYCHROMATES	 1 - 5 		0.01 MG/M3 	Not established	    Not established	  Not established
     13530-65-9
ETHYL BENZENE			0.1-1.0  		100 ppm 		125 ppm		     Not established 	   Not established
     100-41-4
 (As Chromium (VI) Cmpnds)		*		 0.05 mg/m3	 Not established	     Not established	   Not established
    13530-65-9
(As Chromates)			* 		  0.05 mg/m3 	  Not established	      Not established	    Not established
   13530-65-9

Key:         ACGIH=American Conference of Governmental Industrial Hygienists; OSHA=Occupational Safety and Health Administration;
TLV=Threshold Limit Value; TWA=Time Weighted Average; PEL=Permissible Exposure Limit; IPEL=Internal Permissible Exposure Limit; Ceiling=TLV or PEL Ceiling Limit; STEL=TLV or PEL Short-Term Exposure Limit; Skin= Skin Absorption Designation. [C- Ceiling Limit; S-Potential Skin Absorption; R-Respirable Dust]

Additional Information
Not applicable.

SECTION 9 - PHYSICAL & CHEMICAL PROPERTIES

(FORMULA VALUES, NOT SALES SPECIFICATIONS)

SPECIFIC GRAVITY: 		.882 					PHYSICAL STATE: Liquid
PERCENT SOLIDS: 		14.72
PERCENT VOLATILE BY VOLUME: 90.410 				pH: Not available.
SOLUBILITY IN WATER (%):	 65.2 % 				ODOR THRESHHOLD: Not available.
VAPOR PRESSURE (mm Hg): 40.8 mmHg  	ODOR/APPEARANCE: Viscous liquid with an odor characteristic of the solvents listed in Section 2.

VAPOR DENSITY: 		HEAVIER THAN AIR
EVAPORATION RATE:		 222
BOILING POINT OR RANGE: 	149 - 358Degrees F 		FREEZING POINT OR RANGE: Not available.
MELTING POINT OR RANGE: 	 Not available.
OCTANOL/WATER PARTITION COEFFICIENT:    Not available.
WEIGHT PER GALLON: 	7.35 (U.S.) / 8.8 (IMPERIAL)

SECTION 10 - STABILITY AND REACTIVITY

STABILITY:
This product is normally stable and will not undergo hazardous reactions.
CONDITIONS TO AVOID:
None Known.
INCOMPATIBLE MATERIALS:
Avoid contact with strong alkalies, strong mineral acids, or strong oxidizing agents.
HAZARDOUS POLYMERIZATION:
None Known.
HAZARDOUS DECOMPOSITION PRODUCTS:
•Carbon monoxide •Carbon dioxide •Lower molecular weight polymer fractions

SECTION 11 - TOXICOLOGICAL INFORMATION

ACUTE TOXICITY
						ORAL   		DERMAL		INHALATION	
   Material/CAS Number  		Percent    	LD50 (g/kg)	LD50 (g/kg)	LC50 (mg/l)

ETHYL ALCOHOL			40 - 70 		7.06 g/kg 		Not Available	Not Available
         64-17-5
PROPYLENE GLYCOL		  5 - 10 		5.66 g/kg 		  13.00 g/kg 	Not Available
MONOMETHYL ETHER
        107-98-2
TOLUENE			   3 - 7 		5.00 g/kg		  12.12 g/kg 	Not Available
       108-88-3
ISOBUTYL ALCOHOL		   3 - 7 		2.40 g/kg 		    3.40 g/kg 	Not Available
       78-83-1
XYLENES			   1 - 5 		4.30 g/kg		 Not Available	 Not Available
     1330-20-7
ETHYL ACETATE			   1 - 5 		 5.62 g/kg 	 Not Available 	14.41 mg/L. 4 h
     141-78-6
METHYL ALCOHOL		   1 - 5 		 5.63 g/kg 	   15.80 g/kg 	 Not Available
     67-56-1
ETHYL BENZENE			  0.1-1.0 		  3.50 g/kg 	    17.80 g/kg	 Not Available
   100-41-4
CHRONIC TOXICITY

TARGET ORGANS:
•Causes blindness •Carcinogen •Kidney •Liver •Teratogen •Embryo toxin •Brain •Central nervous system •Lung

MUTAGENICITY:
This has not been tested for this product.
REPRODUCTIVE:
This has not been tested for this product.
SUPPLEMENTAL HEALTH INFORMATION:

   Material/CAS Number		Percent		Ingredient Specific Animal Data:		

METHYL ALCOHOL		1 - 5 		Cannot be made non-poisonous
       67-56-1
ETHYL BENZENE			0.1-1.0 	Ethyl benzene has been reported by NTP to cause cancer in laboratory animals
100-41-4	following a chronic (2 year) inhalation exposure. Dose levels of 75, 250 and 750
ppm were used, with evidence of carcinogenicity found in the kidneys of rats and    the lung and liver of mice at 750 ppm. The No Observed Effect Level (NOEL) was 75 ppm. The relevance of these findings to humans is uncertain, but appropriate safeguards should be employed to reduce or eliminate inhalation exposure to ethyl benzene.

SECTION 12 - ECOLOGICAL INFORMATION

POTENTIAL ENVIRONMENTAL EFFECTS:
Ecotoxicity 		No data available

ENVIRONMENTAL FATE
MOBILITY: 		None Known.
BIODEGRADATION: 	None Known.
Bioaccumulation 	No data available

PHYSICAL/CHEMICAL
HYDROLYSIS: 		None Known.
PHOTOLYSIS: 		None Known.

SECTION 13 - DISPOSAL CONSIDERATIONS

Provide maximum ventilation, only personnel equipped with proper respiratory and skin and eye protection should be permitted in the area. Take up spilled material with sawdust, vermiculite, or other absorbent material and place in containers for disposal.
Waste material must be disposed of in accordance with federal, state, provincial and local environmental control
regulations. Empty containers should be recycled by an appropriately licensed reconditioner/salvager or disposed of through a permitted waste management facility. Additional disposal information is contained on the Environmental Data Sheet for this product, which can be obtained from your Air-Tech representative.

SECTION 14 - TRANSPORTATION INFORMATION

Proper Shipping Name: 		Paint
NOS Technical Name: 			None
Hazard Class: 				3
Subsidiary Class(es): 			None
UN Number: 				UN1263
Packing Group: 			II
USA - RQ Hazardous Substances:
Xylenes, Toluene

USA-RQ Hazardous Substance Threshold Ship Weight:
Xylenes>2347.18 Pounds, Toluene>15015.17 Pounds
Marine Pollutant Name:
None
USA Shipments Only - RQ Threshold Ship Weight: This is the total weight of this product that must be shipped to exceed the RQ quantity.

SECTION 15 - REGULATORY INFORMATION

INVENTORY STATUS
U.S. TSCA:       This product and/or all of its components are listed on the U.S. TSCA Inventory or is otherwise exempt from TSCA Inventory reporting requirements.

FEDERAL REGULATIONS

US Regulations

     Material/CAS Number	Percent		CERCLA HS - RQ (LBS) 	SARA EHS-TPQ (LBS) 	SARA 313

TOLUENE		3 - 7 			1000 lbs 		Not Listed 		Listed
   108-88-3
ISOBUTYL ALCOHOL	3 - 7 			5000 lbs 		Not Listed 		Not Listed
    78-83-1
XYLENES		1 - 5 			100 lbs 		Not Listed 		Listed
   1330-20-7
ETHYL ACETATE		1 - 5 			5000 lbs 		Not Listed 		Not Listed
   141-78-6
METHYL ALCOHOL	1 - 5 			5000 lbs 		Not Listed		 Listed
    67-56-1
ETHYL BENZENE		0.1-1.0 			1000 lbs 		Not Listed		 Listed
   100-41-4

SARA 311/312
Health (acute): 		Yes
Health (chronic): 	Yes
Fire (flammable): 	Yes
Pressure: 		No
Reactivity: 		No

WHMIS HAZARD CLASS: •	Class B, Division 2 •Class D, Division 2, Subdivision A •Class D, Division 2,
Subdivision B

STATE/PROVINCIAL REGULATIONS
CALIFORNIA PROP. 65:             WARNING: This product contains a chemical(s) known to the State of California to cause cancer and birth defects or other reproductive harm.

Additional Information

Material/CAS Number		Percent	ARC Group	IARC Group	IARC 2B (	      ACGIH Carc	NTP Known	OSHA Carc.
				1(Known		2A (Probable	Suspected			Carc.
				Human Carc.)	Carc.)		Carc.)					

ZINC TETRA-OXYCHROMATES	1 - 5 	     N 		    N		       N 	              Y	      * Y		      Y
         13530-65-9
ETHYL BENZENE		0.1-1.0	     N 		    N 		       Y	               N 	         N		       N
         100-41-4

Key: 
IARC- International Agency on the Research of Cancer; ACGIH- American Conference of Governmental
Industrial Hygienists; NTP- National Toxicology Program *Denotes chemical as NTP Known Carcinogen; + Denotes NTP Possible Carcinogen;
OSHA-Occupational Safety and Health Administration.

SECTION 16 - OTHER INFORMATION

Hazard Rating Systems
NFPA Rating: 		2 30
HMIS Rating: 		2*30
Rating System: 0=Minimal, 1=Slight, 2=Moderate, 3=Serious, 4=Severe, *=Chronic Effects.
HMIS=Hazardous Materials Identification System; NFPA=National Fire Protection Association;
Safe handling of this product requires that all of the information on the MSDS be evaluated for specific work environments and conditions of use.

PREPARED BY:  AIR TECH COATINGS
REASON FOR REVISION: Date. Edition.
This Material Safety Data Sheet has been prepared in accordance with Canada's Workplace Hazardous Materials
Information System (WHMIS) and the OSHA Hazard Communication Standard (29 CFR 1910.1200), the supplier
notification requirements of SARA Title III, Section 313 and other applicable right-to-know regulations.
Additional environmental and disposal information is contained on the Environmental Data Sheet for this product, which can be obtained from your Air-Tech representative.