COMPANY IDENTITY:  AIR TECH COATINGS, INC.		 Preparation Date: 10/10/10  Supersedes Date:  07/01/09
PRODUCT  IDENTITY:  SPAR VARNISH							PAGE     1

					MATERIAL SAFETY DATA SHEET
THIS MSDS COMPLIES WITH 29 CFR 1910.  1200  (HAZARD COMMUNICATION STANDARD).
IMPORTANT:  Read this MSDS before handling and disposing of this product.  Pass this information on to employees, customers, & users of this product.

			SECTION 1; CHEMICAL PRODUCT AND COMPANY IDENTIFICATION
PRODUCT IDENTITY:  SPAR VARNISH
NAME:  AIR TECH COATINGS, INC.   			     	ADDRESS:  #1 PARADISE PARK RD.
CITY:  JACKSONVILLE, AR 72076			     	PHONE:  1-501-985-1484
							     		INFOTRAC PHONE:  1-800-535-5053

				SECTION 2;  INGREDIENT & REGULATORY INFORMATION
All components of this product are on the TSCA list.
SARA Title III Section 313 Supplier Notification
		This product contains the <*> toxic chemicals subject to the reporting requirements of Section 313 of the Emergency Planning & Community Right-to-Know Act of 1986 & of 40 CFR 372.  This information must be included in all MSDS’s that are copied and distributed for this material.
SARA TITLE III INGREDIENTS			CAS #		WT. %	   (REG. SECTION)  RQ(LBS)
ETHYL ACETATE			141-78-6	NA	    (311, 312)	       NONE	
METHYL n-PROPYL KETONE		107-87-9	NA	    (311, 312)	       NONE
*TOLUENE				108-88-3		    (311, 312, 313, RCRA)  1000
ETHYL-3-ETHOXYPROPIONAT		763-69-9	NA	    (311, 312)	       NONE
*METHYL ISOBUTYL KETONE		108-10-1		    (311, 312, 313, RCRA)  5000
2-Methoxypropyl Acetate (PMA)		108-65-6		    (311, 312, 313, RCRA)
XYLENE				1330-20-7		    (311, 312, 313, RCRA)
POLYESTER RESIN, FILM FORMERS, ADDITIVES            58
SARA SECTION 311/312 HAZARDS:  Acute Health, Fire
MATERIAL				CAS #	       TWA +  (OSHA)	TLV (ACGIH)
ETHYL ACETATE			141-78-6	400 PPM	400 PPM
METHYL N-PROPYL KETONE		107-87-9	200 PPM	200 PPM
TOLUENE				108-88-3	100 PPM	100 PPM
ETHYL-3-ETHOXYPROPIONAT		763-69-9	  50 PPM	  50 PPM
METHYL ISOBUTYL KETONE		108-10-1	  50 PPM	  50 PPM
2-Methoxypropyl Acetate (PMA)		108-65-6	100 PPM	Not est
XYLENE				1330-20-7	100 PPM	100 PPM
MATERIAL 				CAS #		CEILING	STEL (OSHA/ACGIH)
TOLUENE				108-88-3	300 PPM	150 PPM
METHYL ISOBUTYL KETONE		108-10-1	None Known	75 PPM
Xylene					1330-20-7	100 ppm		150 PPM
MATERIAL				CAS #	          LOWEST KNOWN LETHAL DOSE DATA
						          LOWEST KNOWN LD50 (ORAL)
METHYL ISOBUTYL KETONE		108-10-1          2080.0 MG/KG (RATS)
						          LOWEST KNOWN LC50 (VAPORS)
ETHYL ACETATE			141-78-6          1600 PPM (RATS)
						           LOWEST KNOWN LD50 (SKIN)
TOLUENE				108-88-3           4000.0 MG/KG (RABBITS)
HAZARDS:  HEALTH (NFPA) 2     HEALTH (HMIS):  1     FLAMMABILITY:  3   REACTIVITY:  0

COMPANY IDENTITY:  AIR TECH COATINGS, INC.	Preparation Date 07/01/09 Supersedes Date:  06/22/08
PRODUCT IDENTITY:  SPAR VARNISH						PAGE   2

				SECTION 2:  INGREDIENT & REGULATORY INFORMATION
		CALIFORNIA PROPOSITION 65:  This product contains the following chemical known to the state of California to cause reproductive toxicity:
              Toluene
	       DOT SHIPPING NAME:  PAINT RELATED MATERIAL, 3, (UN1263), PG-II
	           DRUM LABEL:  3 (FLAMMABLE LIQUID)

					SECTION 3;  HAZARDS IDENTIFICATION
		THRESHOLD LIMIT VALUE:  140 PPM (EVAPORATED BLEND)
		CONTAINS:  ETHYL ACETATE, METHYL n-PROPYL KETONE, TOLUENE, ETHYL-3-ETHOXYPROPIONAT, METHYL ISOBUTYL KETONE, 2-METHOXYPROPYL ACETATE (PMA), XYLENE
					        	 WARNING!
					       	FLAMMABLE!!
					         -ACUTE HAZARDS
EYE & SKIN CONTACT:
		Primary irritation to skin, defatting, dermatitis.  Adsorption through skin increases exposure.
		Primary irritation to eyes, redness, tearing, blurred vision.
		Liquid can cause eye irritation.  Wash thoroughly after handling.
INHALATION:  
		Anesthetic.  Irritates respiratory tract.  Acute overexposure can cause serious nervous system depression.  Vapor harmful.
		Breathing vapor can cause irritation. 
		Acute overexposure can cause damage to kidneys, blood, nerves, liver, & lungs.
SWALLOWING:
		Harmful or fatal if swallowed.
		Swallowing can cause abdominal irritation, nausea, vomiting, & diarrhea.
				SUBCHRONIC HAZARDS/ CONDITIONS AGGREVATED
SUBCHRONIC HAZARDS
		Absorption through skin may be harmful.  Studies with laboratory animals indicate this product can cause damage to fetus.
		Chronic overexposure can cause damage to kidneys, blood, nerves, liver & lungs.
		Persons with asthma, chronic respiratory problems, severe heart, skin, liver or kidney problems should avoid use.  
						CHRONIC HAZARDS
		This product has no carcinogens listed by 1ARC, NIP, NIOSH, OSHA, or ACGIH, as of this date, greater or equal to 0.1%.
		This product may contain less than 100 ppm of Benzene.
		Not considered in such low concentrations. 

COMPANY IDENTITY:  AIR TECH COATINGS, INC.    Preparation Date 07/01/09 Supersedes Date:  06/22/08
PRODUCT IDENTITY:  SPAR VARNISH						PAGE   3

				SECTION 4;  FIRST AID MEASURES PROCEDURES
EYE CONTACT:
		For eyes, immediately flush with plenty of water for 15 minutes & CALL A PHYSICIAN.
SKIN CONTACT:
		In case of contact with skin, immediately remove contaminated clothing.  Wash thoroughly with soap & water.  Wash contaminated clothing before reuse.     (Discard contaminated shoes.)
INHALATION:  
		After high vapor pressure, remove to fresh air,  If breathing is difficult, give oxygen.  If breathing has stopped give artificial respiration.  CALL        A PHYSICIAN IMMEDIATELY!!
SWALLOWING:
		If swallowed, CALL A PHYSICIAN IMMEDIATELY!  Never give anything by mouth to an unconscious person.
					SECTION 5;  FIRE FIGHTING MEASURES
LOWER FLAMMABLE LIMIT IN AIR (% BY VOLUME):  1.8
FLASH POINT (TEST METHOD):  70 F (PMCC)
FLAMMABILITY CLASSIFICATION:  CLASS I B
EXTINGUISHING MEDIA
		NFPA Class B extinguishers (Carbon Dioxide or foam) for Class I B liquid fires.
SPECIAL FIRE FIGHTING PROCEDURES
		Water spray may be ineffective on fire but can protect fire-fighters & cool closed containers.  Use fog nozzles if water is used.
		Do not enter confined fire-space without full bunker gear.  (Helmet with face shield, bunker coats, gloves & rubber boots).
		Use NIOSH approved positive-pressure self-contained breathing apparatus.
UNUSUAL EXPLOSION AND FIRE PROCEDURES
		FLAMMABLE!!
		Keep container tightly closed.
		Isolate from oxidizers, heat, sparks, electric equipment & open flame.
		Closed containers may explode if exposed to extreme heat.
		Applying to hot surfaces requires special precautions.
		Empty container very hazardous!  Continue all label precautions!!

COMPANY IDENTITY:  AIR TECH COATINGS, INC.	Preparation Date 07/01/09 Supersedes Date: 06/22/08
PRODUCT IDENTITY:  SPAR VARNISH						PAGE   4
				SECTION 6;  ACCIDENTAL RELEASE  MEASURES
SPILL OR LEAK PROCEDURES:
		Stop spill at source.  Dike area & contain.  Clean up area with absorbent materials.  Mop up & dispose of.  Persons without proper protection	        should be kept from area until cleaned up.
WASTE DISPOSAL METHOD:
		Recycle or dispose of observing local, state & Federal health, safety & pollution laws.  If questions exist, contact the appropriate agencies.
OTHER PRECAUTIONS:
		None
				SECTION 7;  HANDLING AND STORAGE
HANDLING
		Isolate from oxidizers, heat, sparks, electric equipment & open flame.  Use only with adequate ventilation.  Avoid breathing of vapor or spray mist.
		Avoid contact with skin & eyes.
		Near OSHA Standard goggles or face shield.  Consult Safety Equipment supplier.
		Wear gloves, apron & footwear impervious to this material.  Wash clothing before reuse.
		Avoid free fall of liquid.  Ground containers when transferring.  Do not flame, cut, saw, drill, braze, or weld.  Emoty container very hazardous!!     Continue all label precautions!
STORAGE
		Do not store above 49 C/120F.  Store large amounts in structures made for OSHA Class I B liquids.  Keep container tightly closed & upright when not in       use to prevent leakage.
			SECTION 8;  EXPOSURE CONTROLS/ PERSONAL PROTECTION:
EXPOSURE CONTROLS:
		Ventilate to keep vapors of this material below 70 ppm.  If over TLV, in accordance with 29 CFR 1910.134, use NIOSH approved positive-pressure self       contained breathing apparatus.  Consult Safety Equipment Supplier.  Use explosion-proof equipment.
VENTILATION:  
		LOCAL EXHAUST			:  NECESSARY
		MECHANICAL (GENERAL)		:  ACCEPTABLE
		SPECIAL				:  NONE
		OTHER					:  NONE
PERSONAL PROTECTIONS:
		Wear OSHA Standard goggles or face shield.  Consult Safety Equipment Supplier.
		Wear gloves, apron & footwear impervious to this material.  Wash clothing before reuse.

COMPANY IDENTITY:  AIR TECH COATINGS, INC.     Preparation Date 07/01/09 Supersedes Date:  06/22/08   
PRODUCT IDENTITY:  SPAR VARNISH						PAGE   5
					SECTION 9;  PHYSICAL DATA
APPEARANCE:  						LIQUID, WATER WHITE
ODOR:								KETONE
BOILING RANGE:						76  103  166  C  /  170  218  331  F
GRAVITY @ 60F:						
	          	          API:							     32.2
	          	          SPECIFIC GRAVITY (WATER=1)				     1.036
	           	           POUNDS/GALLON  :					      8.63
VOC’S (VAPOR PRESSURE   >0.44 LBS/SQ  IN) (LBS/GAL)	                     3.58
TOTAL NONVOLATILE ORGANIC COMPOUNDS (TVOC)  (G/L):	                    472
NONEXPEMPT VOLATILE ORGANIC COMPOUNDS (CVOC) (G/L):                472
NONEXEMPT VOLATILE ORGANIC COMPOUNDS (CVOC)  (VOL %)              53.2
VAPOR PRESSURE  (MM OF HG) @20C					       43.0
VAPOR DENSITY (AIR=1)						        3.4
WATER ABSORPTION  :						   APPRECIABLE
% VOLATILE BY VOLUME  :						      53.2
				SECTION 10;  REACTIVITY DATA
STABILITY
		Stable
CONDITIONS TO AVOID
		Isolate from oxidizers, heat, sparks, electric equipment & open flame.
MATERIALS TO AVOID
		Isolate from strong oxidizers such as permanganates, chromates and peroxides.
HAZARDOUS DECOMPOSITION PRODUCTS
		Carbon Monoxide, Carbon Dioxide from burning.
HAZARDOUS POLYMERIZATION
		Will not occur.

						NOTICE
Supplier disclaims all expressed or implied warranties of merchantability or fitness for a specific use, with respect to the product or the information provided herein, except for confirmation to contracted specifications.
All information appearing herein is based upon data obtained from manufacturers and/or recognized technical sources.  While this information is believed to be accurate, we make no representations as to its accuracy or sufficiency.
Conditions of use are beyond our control, and therefore users are responsible for verifying the data under their own operating conditions to determine whether the product is suitable for their particular purposes and they assume all risks of their use, handling and disposal of the product.  Users also assume all risks in regards to the publication or use of, or reliance upon information contained herein.
This information relates only to the product designated herein, and does not relate to its use in combination with any other materials or process.